| ## Moving Coil (Needle Instruments)
(1) The example shows the Moving Coil instrument in PPM mode with vertical Stereo arrangement (separate display for left and right channel). Move the mouse accross the display elements to get the corresponding descriptions.
(2) The example shows the Moving Coil instrument in VU mode with vertical Stereo arrangement (separate display for left and right channel). Move the mouse accross the display elements to get the corresponding descriptions.
(3) The example shows the Moving Coil instrument in PPM + Loudness mode with horizontal Dual arrangement (left and right channel in one display with additional loudness display). Move the mouse accross the display elements to get the corresponding descriptions.
The Moving Coil instrument is only available for audio groups with Mono or Stereo signals and can be used instead of the PPM instrument with bargraph display. It features a genuine emulation of various moving coil level meter types. Using the modes PPM (1) with different selectable British scales or VU (2) with adjustable lead, the L and R channels of a stereo signal can be displayed in one single (L/R or M/S) or two separate moving coil instruments. If two separate instruments are used, they may be displayed in horizontal or vertical arrangements (see examples). Similar to this, mode Loudness with a scale according to the selected loudness standard can be used when licence SW20002 is activated. With SW20002, mode PPM + Loudness provides a combination of stereo PPM and summed loudness meter (BBC mode) (3). This kind of instrument includes the PPM with different selectable British scales and its two needles for L (red) and R (green) in horizontal dual arrangement and an additional scale with a cyan-coloured needle to display one of the selectable summing loudness values M, S or I. The center of the fixed relative loudness scale (–9 to +9) represents the target level of the selected loudness standard, the green marked section the tolerance range.