| ## AES Status
Move the mouse accross the display elements to get the corresponding descriptions.
The AES status monitor displays the status bytes from the AES/EBU data stream as plain text or binary data and gives a range of signal status information. The display of the audio data bits and their activity is useful when you need to determine the word width or identify defective bits in the data stream.