| ## Stereo Correlator
Move the mouse accross the display elements to get the corresponding descriptions.
Identical signals in both channels have a correlation of +1; completely unrelated signals have a correlation of 0. Normal stereo mixes mostly show correlation values between 0.3 and 0.7. When both channels carry identical signals but one channel's polarity is switched (180° phase), the correlation will be -1. When analyzing audio using the Correlator, please ensure that the display does not read negative values (shown in red) across extended periods.